{"text_format":"2","workbook":"xlsx","n_sheets":4,"sheets":["Sheet1","DI-DO","AO","AI"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":4,"n_cols":4,"rows_kept":4,"cut":false,"hidden":false,"merged":[]}
[null,null,null,"PLC TO PC ==AI"]
[null,null,null,"PC TO PLC ==AO"]
[null,null,null,"DI== PLC TO PC"]
[null,null,null,"DO== PC TO PLC"]

{"sheet":"DI-DO","index":1,"n_rows":244,"n_cols":15,"rows_kept":244,"cut":false,"hidden":false,"merged":[]}
["DI","Name","Note","Postion (NO Power)","Location","Logic Note",null,null,"#.DO","ID","Name","EV No.","Note","Location","Logic Note"]
["DI-00","Signal_LS-IN motor origin","M0进料升降马达原点信号",null,"W0.00","1==on ,0==off",null,null,"DO-00",null,"Brake relay_LS-IN",null,"进料升降台刹车继电器","W10.00","1== 松开,0== 刹住"]
["DI-01","Signal_LS-IN motor CW limit ","M0进料升降马达CW限位信号",null,"W0.01","1==normal ,0== error",null,null,"DO-01",null,"Brake relay_LS-OUT",null,"出料升降台刹车继电器","W10.01","1== 松开,0== 刹住"]
["DI-02","Signal_LS-IN motor CCW limit ","M0进料升降马达CCW限位信号",null,"W0.02","1==normal ,0== error",null,null,"DO-02",null,"Motor M0 ON_LS-IN",null,"进料升降台马达M0伺服ON","W10.02","1== on,0== off"]
["DI-03","Signal_LS-OUT motor origin","M1出料升降马达原点信号",null,"W0.03","1==on ,0== off",null,null,"DO-03",null,"Motor M1 ON_LS-OUT",null,"出料升降台马达M1伺服ON","W10.03","1== on,0== off"]
["DI-04","Signal_LS-OUT motor CW limit ","M1出料升降马达CW限位信号",null,"W0.04","1==normal ,0== error",null,null,"DO-04",null,"Motor M2 ON_PB-CHB",null,"进料拨杆马达M2伺服ON","W10.04","1== on,0== off"]
["DI-05","Signal_LS-OUT motor CCW limit ","M1出料升降马达CCW限位信号",null,"W0.05","1==normal ,0== error",null,null,"DO-05",null,"Motor M3 ON_PB-IN",null,"进料推杆马达M3伺服ON","W10.05","1== on,0== off"]
["DI-06","Signal_PB-CHB origin","M2腔体拨杆马达原点信号",null,"W0.06","1==on ,0==off",null,null,"DO-06",{"$nulls":4},"W10.06"]
["DI-07","Sensor_PB-CHB CW limit ","M2腔体拨杆CW限位传感器",null,"W0.07","1==normal ,0== error",null,null,"DO-07",null,"PB-CHB U&D cylinder",null,"腔体拨杆上下气缸","W10.07","1== 下,0==上"]
["DI-08","Sensor_PB-CHB CCW limit ","M2腔体拨杆CCW限位传感器",null,"W0.08","1==normal ,0== error",null,null,"DO-08",null,"R-IN U&D cylinder",null,"进料轨道止档气缸","W10.08","1== 上,0== 下"]
["DI-09","Signal_PB-IN origin","M3进料推杆马达原点信号",null,"W0.09","1==on,0== off",null,null,"DO-09",null,"R-IN L&R cylinder",null,"进料轨道左右平移气缸","W10.09","1== 右,0==左"]
["DI-10","Sensor_PB-IN CW limit ","M3进料推杆CW限位传感器",null,"W0.10","1==normal ,0== error",null,null,"DO-10",null,"R-IN motor relay",null,"进料轨道马达继电器","W10.10","1==on,0==off"]
["DI-11","Sensor_PB-IN CCW limit ","M3进料推杆CCW限位传感器",null,"W0.11","1==normal ,0== error",null,null,"DO-11",null,"PB-OUT U&D cylinder",null,"出料拨杆上下气缸","W10.11","1== 下,0==上"]
["DI-12","Signal_LS-IN locating complete","进料升降马达驱动器定位完成信号(驱动器)",null,"W0.12","1==ok ,0== no",null,null,"DO-12",null,"PB-OUT F&B cylinder",null,"出料拨杆前后气缸","W10.12","1==右,0==左"]
["DI-13","Signal_LS-IN alarm ","进料升降马达驱动器报警信号(驱动器)",null,"W0.13","1==normal ,0== error",null,null,"DO-13",null,"R-OUT U&D cylinder",null,"出料轨道止档气缸","W10.13","1== 上,0== 下"]
["DI-14","Signal_LS-OUT locating complete","出料升降马达驱动器定位完成信号(驱动器)",null,"W0.14","1==ok ,0== no",null,null,"DO-14",null,"R-OUT L&R cylinder",null,"出料轨道左右平移气缸","W10.14","1== 右,0==左"]
["DI-15","Signal_LS-OUT alarm ","出料升降马达驱动器报警信号(驱动器)",null,"W0.15","1==normal ,0== error",null,null,"DO-15",null,"R-OUT motor relay",null,"出料轨道马达继电器","W10.15","1==on,0==off"]
["DI-16","Signal_PB-CHB locating complete","进料拨杆马达驱动器定位完成信号(驱动器)",null,"W1.00","1==ok ,0== no",null,null,"DO-16",null,"LS-IN M0 manual operate rising",null,"进料升降台M0手动上升","W11.00","1==on,0==off"]
["DI-17","Signal_PB-CHB alarm ","进料拨杆马达驱动器报警信号(驱动器)",null,"W1.01","1==normal ,0== error",null,null,"DO-17",null,"LS-IN M0 manual operate declining",null,"进料升降台M0手动下降","W11.01","1==on,0==off"]
["DI-18","Signal_PB-IN locating complete","进料推杆马达驱动器定位完成信号(驱动器)",null,"W1.02","1==ok ,0== no",null,null,"DO-18",null,"LS-OUT M1 manual operate rising",null,"出料升降台M1手动上升","W11.02","1==on,0==off"]
["DI-19","Signal_PB-IN alarm ","进料推杆马达驱动器报警信号(驱动器)",null,"W1.03","1==normal ,0== error",null,null,"DO-19",null,"LS-OUT M1 manual operate declining",null,"出料升降台M1手动下降","W11.03","1==on,0==off"]
["DI-20","Sensor_PB-IN prevent sticking","进料推杆防卡传感器",null,"W1.04","0==normal ,1== error",null,null,"DO-20",null,"PB-CHB M2 manual operate moving left",null,"进料拨杆M2手动向左","W11.04","1==on,0==off"]
["DI-21","Sensor_PB-CHB prevent sticking","腔体拨杆防卡传感器",null,"W1.05","0==normal ,1== error",null,null,"DO-21",null,"PB-CHB M2 manual operate moving right",null,"进料拨杆M2手动向右","W11.05","1==on,0==off"]
["DI-22","Sensor_PB-OUT prevent sticking","出料拨杆防卡传感器",null,"W1.06","0==normal ,1== error",null,null,"DO-22",null,"PB-IN M3 manual operate moving left",null,"进料推杆M3手动向左","W11.06","1==on,0==off"]
["DI-23","Sensor_R4-IN entrance","进料前轨道入口传感器",null,"W1.07","1==on ,0== off",null,null,"DO-23",null,"PB-IN M3 manual operate moving right",null,"进料推杆M3手动向右","W11.07","1==on,0==off"]
["DI-24","Sensor_R4-IN stop bit","进料前轨道停止位传感器",null,"W1.08","1==on ,0== off",null,null,"DO-24",null,"LS-IN MGZ go to M0 location",null,"去M0进料盒指定位置","W11.08","1==on,0==off"]
["DI-25","Sensor_R3-IN entrance","进料中前轨道入口传感器",null,"W1.09","1==on ,0== off",null,null,"DO-25",null,"LS-OUT MGZ go to M1 location",null,"去M1出料盒指定位置","W11.09","1==on,0==off"]
["DI-26","Sensor_R3-IN stop bit","进料中前轨道停止位传感器",null,"W1.10","1==on ,0== off",null,null,"DO-26",null,"PB-CHB go to M2 location",null,"去M2进料拨杆指定位置","W11.10","1==on,0==off"]
["DI-27","Sensor_R2-IN entrance","进料中后轨道入口传感器",null,"W1.11","1==on ,0== off",null,null,"DO-27",null,"PB-IN go to M3 location",null,"去M3进料推杆指定位置","W11.11","1==on,0==off"]
["DI-28","Sensor_R2-IN stop bit","进料中后轨道停止位传感器",null,"W1.12","1==on ,0== off",null,null,"DO-28",null,"M0 deviation counter reset",null,"M0偏差计数器复位","W11.12","1==on,0==off"]
["DI-29","Sensor_R1-IN entrance","进料后轨道入口传感器",null,"W1.13","1==on ,0== off",null,null,"DO-29",null,"M1 deviation counter reset",null,"M1偏差计数器复位","W11.13","1==on,0==off"]
["DI-30","Sensor_R1-IN stop bit","进料后轨道停止位传感器",null,"W1.14","1==on ,0== off",null,null,"DO-30",null,"M2 deviation counter reset",null,"M2偏差计数器复位","W11.14","1==on,0==off"]
["DI-31","Sensor_PB-CHB U&D cylinder A top ","进料拨杆上下气缸A上位传感器",null,"W1.15","1==on ,0== off",null,null,"DO-31",null,"M3 deviation counter reset",null,"M3偏差计数器复位","W11.15","1==on,0==off"]
["DI-32","Sensor_PB-CHB U&D cylinder A bottom ","进料拨杆上下气缸A下位传感器",null,"W2.00","1==on ,0== off",null,null,"DO-32",null,"M0 Driver alarm reset",null,"M0驱动器报警复位","W12.00","1== en,0== close"]
["DI-33","Sensor_R-IN L&R cylinder left ","进料轨道左右平移气缸左位传感器",null,"W2.01","1==on ,0== off",null,null,"DO-33",null,"M1 Driver alarm reset",null,"M1驱动器报警复位","W12.01","1== en,0== close"]
["DI-34","Sensor_R-IN L&R cylinder right ","进料轨道左右平移气缸右位传感器",null,"W2.02","1==on ,0== off",null,null,"DO-34",null,"M2 Driver alarm reset",null,"M2驱动器报警复位","W12.02","1== en,0== close"]
["DI-35","Sensor_R-IN U&D cylinder top ","进料轨道止档气缸上位传感器",null,"W2.03","1==on ,0== off",null,null,"DO-35",null,"M3 Driver alarm reset",null,"M3驱动器报警复位","W12.03","1== en,0== close"]
["DI-36","Sensor_R-IN U&D cylinder bottom ","进料轨道止档气缸下位传感器",null,"W2.04","1==on ,0== off",null,null,"DO-36",null,"M0 manual operate stop rising ",null,"M0手动上升停止","w12.04","1== en,0== close"]
["DI-37","Sensor_LS-IN MGZ4","进料前料盒检测传感器",null,"W2.05","1==on ,0== off",null,null,"DO-37",null,"M0 manual operate stop declining",null,"M0手动下降停止","w12.05","1== en,0== close"]
["DI-38","Sensor_LS-IN MGZ3","进料中前料盒检测传感器",null,"W2.06","1==on ,0== off",null,null,"DO-38",null,"M1 manual operate stop rising",null,"M1手动上升停止","w12.06","1== en,0== close"]
["DI-39","Sensor_LS-IN MGZ2","进料中后料盒检测传感器",null,"W2.07","1==on ,0== off",null,null,"DO-39",null,"M1 manual operate stop declining",null,"M1手动下降停止","w12.07","1== en,0== close"]
["DI-40","Sensor_LS-IN MGZ1","进料后料盒检测传感器",null,"W2.08","1==on ,0== off",null,null,"DO-40",null,"M2 manual operate stop moving left",null,"M2手动向左停止","w12.08","1== en,0== close"]
["DI-41","Sensor_R4-OUT entrance","出料前轨道入口传感器",null,"W2.09","1==on ,0== off",null,null,"DO-41",null,"M2 manual operate stop moving right",null,"M2手动向右停止","w12.09","1== en,0== close"]
["DI-42","Sensor_R4-OUT stop bit","出料前轨道停止位传感器",null,"W2.10","1==on ,0== off",null,null,"DO-42",null,"M3 manual operate stop moving left",null,"M3手动向左停止","w12.10","1== en,0== close"]
["DI-43","Sensor_R4-OUT exit","出料前轨道出口传感器",null,"W2.11","1==on ,0== off",null,null,"DO-43",null,"M3 manual operate stop moving right",null,"M3手动向右停止","w12.11","1== en,0== close"]
["DI-44","Sensor_R3-OUT entrance","出料中前轨道入口传感器",null,"W2.12","1==on ,0== off",null,null,"DO-44",null,"M0 looking for origin",null,"M0搜索原点","w12.12","1== en,0== close"]
["DI-45","Sensor_R3-OUT stop bit","出料中前轨道停止位传感器",null,"W2.13","1==on ,0== off",null,null,"DO-45",null,"M1 looking for origin",null,"M1搜索原点","w12.13","1== en,0== close"]
["DI-46","Sensor_R3-OUT exit","出料中前轨道出口传感器",null,"W2.14","1==on ,0== off",null,null,"DO-46",null,"M2 looking for origin",null,"M2搜索原点","w12.14","1== en,0== close"]
["DI-47","Sensor_R2-OUT entrance","出料中后轨道入口传感器",null,"W2.15","1==on ,0== off",null,null,"DO-47",null,"M3 looking for origin",null,"M3搜索原点","w12.15","1== en,0== close"]
["DI-48","Sensor_R2-OUT stop bit","出料中后轨道停止位传感器",null,"W3.00","1==on ,0== off",null,null,"DO-48",null,"TM_Init",null,"TM区域手动初始化","w13.00","1== en,0== close"]
["DI-49","Sensor_R2-OUT exit","出料中后轨道出口传感器",null,"W3.01","1==on ,0== off",null,null,"DO-49",null,"TM_reset（PC）",null,"故障清除","w13.01","1== en,0== close"]
["DI-50","Sensor_R1-OUT entrance","出料后轨道入口传感器",null,"W3.02","1==on ,0== off",null,null,"DO-50",null,"Load Station In Clear Error",null,"进料升降台故障清除","w13.02","1==on,0==off"]
["DI-51","Sensor_R1-OUT stop bit","出料后轨道停止位传感器",null,"W3.03","1==on ,0== off",null,null,"DO-51",null,"PM Clear Error",null,"进料拨杆故障清除","w13.03","1==on,0==off"]
["DI-52","Sensor_R1-OUT exit","出料后轨道出口传感器",null,"W3.04","1==on ,0== off",null,null,"DO-52",null,"Load Station Out Clear Error",null,"出料升降台故障清除","w13.04","1==on,0==off"]
["DI-53","Sensor_PB-OUT U&D cylinder A top ","出料拨杆上下气缸A上位传感器",null,"W3.05","1==on ,0== off",null,null,"DO-53",null,"ask  feeding ",null,"空闲状态请求进料或出料","w13.05","按逻辑"]
["DI-54","Sensor_PB-OUT U&D cylinder A bottom ","出料拨杆上下气缸A下位传感器",null,"W3.06","1==on ,0== off",null,null,"DO-54",null,"ask discharge ",null,"腔体已打开，加工完成请求出料","w13.06","按逻辑"]
["DI-55","Sensor_PB-OUT L&R cylinder left ","出料拨杆左右气缸左位传感器",null,"W3.07","1==on ,0== off",null,null,"DO-55",null,"chamber opened",null,"腔体已打开，且无关闭动作","w13.07","按逻辑"]
["DI-56","Sensor_PB-OUT L&R cylinder right ","出料拨杆左右气缸右位传感器",null,"W3.08","1==on ,0== off",null,null,"DO-56",null,"chamber closed",null,"腔体已关闭，且无打开动作","w13.08","按逻辑"]
["DI-57","Sensor_R-OUT L&R cylinder left ","出料轨道左右平移气缸左位传感器",null,"W3.09","1==on ,0== off",null,null,"DO-57",null,"Safe door  singal work",null,"安全门信号有效","w13.09","按传动参数界面设定"]
["DI-58","Sensor_R-OUT L&R cylinder right ","出料轨道左右平移气缸右位传感器",null,"W3.10","1==on ,0== off",null,null,"DO-58",null,null,null,"备用","w13.10"]
["DI-59","Sensor_R-OUT U&D cylinder top ","出料止档气缸上位传感器",null,"W3.11","1==on ,0== off",null,null,"DO-59",null,null,null,"备用","w13.11"]
["DI-60","Sensor_R-OUT U&D cylinder bottom ","出料止档气缸下位传感器",null,"W3.12","1==on ,0== off",null,null,"DO-60",null,null,null,"备用","w13.12"]
["DI-61","Sensor_LS-OUT MGZ4","出料前料盒检测传感器",null,"W3.13","1==on ,0== off",null,null,"DO-61",null,null,null,"备用","w13.13"]
["DI-62","Sensor_LS-OUT MGZ3","出料中前料盒检测传感器",null,"W3.14","1==on ,0== off",null,null,"DO-62",null,null,null,"备用","w13.14"]
["DI-63","Sensor_LS-OUT MGZ2","出料中后料盒检测传感器",null,"W3.15","1==on ,0== off",null,null,"DO-63",null,null,null,"备用","w13.15"]
["DI-64","Sensor_LS-OUT MGZ1","出料后料盒检测传感器",null,"W4.00","1==on ,0== off",null,null,"DO-64",null,"LS-IN Motor operate stop",null,"M0手动定位停止","w14.00","1== en,0== close,收到FB后off"]
["DI-65","Sign_LS-IN motor M0 pulse output complete","进料升降马达M0脉冲输出完成标志(PLC信号)",null,"W4.01","1==ok ,0== no",null,null,"DO-65",null,"LS-OUT Motor operate stop",null,"M1手动定位停止","w14.01","1== en,0== close,收到FB后off"]
["DI-66","Sign_LS-OUT motor M1 pulse output complete","出料升降马达M1脉冲输出完成标志(PLC信号)",null,"W4.02","1==ok ,0== no",null,null,"DO-66",null,"PB-CHB Motor operate stop",null,"M2手动定位停止","w14.02","1== en,0== close,收到FB后off"]
["DI-67","Sign_PB-CHB motor M2 pulse output complete","进料拨杆马达M2脉冲输出完成标志(PLC信号)",null,"W4.03","1==ok ,0== no",null,null,"DO-67",null,"PB-IN Motor operate stop",null,"M3手动定位停止","w14.03","1== en,0== close,收到FB后off"]
["DI-68","Sign_PB-IN motor M3 pulse output complete","进料推杆马达M3脉冲输出完成标志(PLC信号)",null,"W4.04","1==ok ,0== no",null,null,"DO-68",null,"TM_Ask auto model",null,"请求进入自动模式","w14.04","1== en,0== close,收到FB后off"]
["DI-69","Sign_LS-IN motor outputting M0 pulse ","进料升降马达M0脉冲输出中标志(PLC信号)",null,"W4.05","1==on ,0== off",null,null,"DO-69",null,"TM_Ask manual model",null,"请求进入手动模式","w14.05","1== en,0== close,收到FB后off"]
["DI-70","Sign_LS-OUT motor outputting M1 pulse ","出料升降马达M1脉冲输出中标志(PLC信号)",null,"W4.06","1==on ,0== off",null,null,"DO-70",null,"TM_Ask  auto start",null,"请求自动开始","w14.06","1== en,0== close,收到FB后off"]
["DI-71","Sign_PB-CHB motor outputting M2 pulse ","进料拨杆马达M2脉冲输出中标志(PLC信号)",null,"W4.07","1==on ,0== off",null,null,"DO-71",null,"TM_Ask  auto stop",null,"请求自动停止","w14.07","1== en,0== close,收到FB后off"]
["DI-72","Sign_PB-IN motor outputting M3 pulse ","进料推杆马达M3脉冲输出中标志(PLC信号)",null,"W4.08","1==on ,0== off",null,null,"DO-72",null,"change LS-IN number of plies",null,"确认变更自动M0工作层数","w14.08","1== en,0== close,收到FB后off"]
["DI-73","Sign_LS-IN motor with origin ","进料升降马达M0原点已建立",null,"W4.09","1==origin ,0== no",null,null,"DO-73",null,"change LS-OUT  number of plies",null,"确认变更自动M1工作层数","w14.09","1== en,0== close,收到FB后off"]
["DI-74","Sign_LS-OUT motor with origin ","出料升降马达M1原点已建立",null,"W4.10","1==origin ,0== no",null,null,"DO-74",null,"LS-IN  Positioning target floor",null,"M0手动定位到目标层数","w14.10","1== en,0== close,收到FB后off"]
["DI-75","Sign_PB-CHB motor with origin ","进料拨杆马达M2原点已建立",null,"W4.11","1==origin ,0== no",null,null,"DO-75",null,"LS-OUT Positioning target floor",null,"M1手动定位到目标层数","w14.11","1== en,0== close,收到FB后off"]
["DI-76","Sign_PB-IN motor with origin ","进料推杆马达M3原点已建立",null,"W4.12","1==origin ,0== no",null,null,"DO-76",null,"Confirm material has been cleared",null,"确认设备上的料板已被清除","w14.12","1== en,0== close,收到FB后off"]
["DI-77","Sign_LS-IN motor M0 locating complete","进料升降马达M0定位完成标志(PLC信号)",null,"W4.13","1==ok ,0== no",null,null,"DO-77",null,"recipe  uploaded",null,"配方上传成功","w14.13","1== en,0== close,收到FB后off"]
["DI-78","Sign_LS-OUT motor M1 locating complete","出料升降马达M1定位完成标志(PLC信号)",null,"W4.14","1==ok ,0== no",null,null,"DO-78",{"$nulls":4},"w14.14"]
["DI-79","Sign_PB-CHB motor M2 locating complete","进料拨杆马达M2定位完成标志(PLC信号)",null,"W4.15","1==ok ,0== no"]
["DI-80","Sign_PB-IN motor M3 locating complete","进料推杆马达M3定位完成标志(PLC信号)",null,"W5.00","1==ok ,0== no"]
["DI-81","EMO","急停信号",null,"W5.01"]
["DI-82","Safe Interlock","安全门",null,"W5.02"]
["DI-83",null,null,null,"W5.03"]
["DI-84",null,null,null,"W5.04"]
["DI-85","Sensor_PB-CHB U&D cylinder B top ","进料拨杆上下气缸B上位传感器",null,"W5.05","1==on ,0== off"]
["DI-86","Sensor_PB-CHB U&D cylinder B bottom ","进料拨杆上下气缸B下位传感器",null,"W5.06","1==on ,0== off"]
["DI-87","Sensor_PB-OUT U&D cylinder B top ","出料拨杆上下气缸B上位传感器",null,"W5.07","1==on ,0== off"]
["DI-88","Sensor_PB-OUT U&D cylinder B bottom ","出料拨杆上下气缸B下位传感器",null,"W5.08","1==on ,0== off"]
["DI-89","Init Completed","系统复位完成标志",null,"W5.09","1==ok ,0== no"]
["DI-90","Motor M0 ON_LS-IN FB","进料升降台马达M0伺服ON标志",null,"W5.10","1==ok ,0== no"]
["DI-91","Motor M1 ON_LS-OUT FB","出料升降台马达M1伺服ON标志",null,"W5.11","1==ok ,0== no"]
["DI-92","Motor M2 ON_PB-CHB FB","进料拨杆马达M2伺服ON标志",null,"W5.12","1==ok ,0== no"]
["DI-93","Motor M3 ON_PB-IN FB","进料推杆马达M3伺服ON标志",null,"W5.13","1==ok ,0== no"]
["DI-94",null,null,null,"W5.14"]
["DI-95",null,null,null,"W5.15"]
["DI-96","Signal_LS-IN alarm SW","M0驱动器警告信号（软件）",null,"W6.00","1==alarm ,0== normal"]
["DI-97","Signal_LS-IN alarm HW","M0驱动器报警信号 (硬件）",null,"W6.01","1==alarm ,0== normal"]
["DI-98","Signal_LS-OUT alarm SW","M1驱动器警告信号（软件）",null,"W6.02","1==alarm ,0== normal"]
["DI-99","Signal_LS-OUT alarm HW","M1驱动器错误信号 (硬件）",null,"W6.03","1==alarm ,0== normal"]
["DI-100","Signal_PB-CHB alarm SW","M2驱动器警告信号（软件）",null,"W6.04","1==alarm ,0== normal"]
["DI-101","Signal_PB-CHB alarm HW","M2驱动器错误信号 (硬件）",null,"W6.05","1==alarm ,0== normal"]
["DI-102","Signal_PB-IN alarm SW","M3驱动器警告信号（软件）",null,"W6.06","1==alarm ,0== normal"]
["DI-103","Signal_PB-IN alarm HW","M3驱动器错误信号 (硬件）",null,"W6.07","1==alarm ,0== normal"]
["DI-104","TM_Auto Model ","TM区域进入自动模式",null,"W6.08","1==ok ,0== no"]
["DI-105","TM_Manual  Model ","TM区域进入手动模式",null,"W6.09","1==ok ,0== no"]
["DI-106","TM_Alarm  Model","TM区域发生错误",null,"W6.10","1==ok ,0== no"]
["DI-107","TM_Auto Running","TM区域自动运行中",null,"W6.11","1==ok ,0== no"]
["DI-108","Point  Replace the feeding box","进料口料箱产品已空，请更换",null,"W6.12","1==ok ,0== no"]
["DI-109","Point  Replace the  Finished product box","出料口料箱产品已满，请更换",null,"W6.13","1==ok ,0== no"]
["DI-110","Feeding complete","产品已推入腔体内，且推杆已退出",null,"W6.14","1==ok ,0== no"]
["DI-111","Discharge finish","产品已从腔体推出，且推杆已退出",null,"W6.15","1==ok ,0== no"]
["DI-112",null,"备用",null,"W7.00"]
["DI-113",null,"备用",null,"W7.01"]
["DI-114",null,"备用",null,"W7.02"]
["DI-115",null,"备用",null,"W7.03"]
["DI-116",null,"备用",null,"W7.04"]
["DI-117",null,"备用",null,"W7.05"]
["DI-118",null,"备用",null,"W7.06"]
["DI-119",null,"备用",null,"W7.07"]
["DI-120",null,"备用",null,"W7.08"]
["DI-121",null,"备用",null,"W7.09"]
["DI-122",null,"备用",null,"W7.10"]
["DI-123",null,"备用",null,"W7.11"]
["DI-124","Fb_M0 looking for origin","M0手动找原点请求反馈",null,"W7.12"]
["DI-125","Fb_M1 looking for origin","M1手动找原点请求反馈",null,"W7.13"]
["DI-126","Fb_M2 looking for origin","M2手动找原点请求反馈",null,"W7.14"]
["DI-127","Fb_M3 looking for origin","M3手动找原点请求反馈",null,"W7.15"]
["DI-128","Fb_LS-IN Motor operate stop","M0手动定位停止反馈",null,"W8.00"]
["DI-129","Fb_LS-OUT Motor operate stop","M1手动定位停止反馈",null,"W8.01"]
["DI-130","Fb_PB-CHB Motor operate stop","M2手动定位停止反馈",null,"W8.02"]
["DI-131","Fb_PB-IN Motor operate stop","M3手动定位停止反馈",null,"W8.03"]
["DI-132","Fb_TM_Ask auto model","请求进入自动模式反馈",null,"W8.04"]
["DI-133","Fb_TM_Ask manual model","请求进入手动模式反馈",null,"W8.05"]
["DI-134","Fb_TM_Ask  auto start","请求自动开始反馈",null,"W8.06"]
["DI-135","Fb_TM_Ask  auto stop","请求自动停止反馈",null,"W8.07"]
["DI-136","Fb_change LS-IN number of plies","确认变更自动M0工作层数反馈",null,"W8.08"]
["DI-137","Fb_change LS-OUT  number of plies","确认变更自动M1工作层数反馈",null,"W8.09"]
["DI-138","Fb_LS-IN  Positioning target floor","M0手动定位到目标层数反馈",null,"W8.10"]
["DI-139","Fb_LS-OUT Positioning target floor","M1手动定位到目标层数反馈",null,"W8.11"]
["DI-140","Confirm material has been cleared","确认设备上的料板已被清除反馈",null,"W8.12"]
["DI-141","recipe  uploaded","配方上传成功反馈",null,"W8.13"]
["DI-142",null,null,null,"W8.14"]
["DI-143",null,null,null,"W8.15"]
["DI-144",null,null,null,"W9.00"]
["DI-145",null,null,null,"W9.01"]
["DI-146",null,null,null,"W9.02"]
["DI-147",null,null,null,"W9.03"]
["DI-148",null,null,null,"W9.04"]
["DI-149",null,null,null,"W9.05"]
["DI-150",null,null,null,"W9.06"]
["DI-151",null,null,null,"W9.07"]
["DI-152",null,null,null,"W9.08"]
["DI-153",null,null,null,"W9.09"]
["DI-154",null,null,null,"W9.10"]
["DI-155",null,null,null,"W9.11"]
["DI-156",null,null,null,"W9.12"]
["DI-157",null,null,null,"W9.13"]
["DI-158",null,null,null,"W9.14"]
["DI-159",null,null,null,"W9.15"]
["DI-160","LS-IN motor alarm","进料升降伺服M0异常报警",null,"W20.00"]
["DI-161","LS-OUT motor alarm","出料升降伺服M1异常报警",null,"W20.01"]
["DI-162","PB-CHB motor alarm","腔体拨杆伺服M2异常报警",null,"W20.02"]
["DI-163","PB-IN motor alarm","进料推杆伺服M3异常报警",null,"W20.03"]
["DI-164","LS-IN motor CW limit alarm","进料升降伺服M0正限位触碰报警",null,"W20.04"]
["DI-165","LS-OUT motor CW limit alarm","出料升降伺服M1正限位触碰报警",null,"W20.05"]
["DI-166","PB-CHB motor CW limit alarm","腔体拨杆伺服M2正限位触碰报警",null,"W20.06"]
["DI-167","PB-IN motor CW limit alarm","进料推杆伺服M3正限位触碰报警",null,"W20.07"]
["DI-168","LS-IN motor CCW limit alarm","进料升降伺服M0负限位触碰报警",null,"W20.08"]
["DI-169","LS-OUT motor CCW limit alarm","出料升降伺服M1负限位触碰报警",null,"W20.09"]
["DI-170","PB-CHB motor CCW limit alarm","腔体拨杆伺服M2负限位触碰报警",null,"W20.10"]
["DI-171","PB-IN motor CCW limit alarm","进料推杆伺服M3负限位触碰报警",null,"W20.11"]
["DI-172","LS-IN motor origin fail alarm","进料升降伺服M0找原点失败报警",null,"W20.12"]
["DI-173","LS-OUT motor ORG fail alarm","出料升降伺服M1找原点失败报警",null,"W20.13"]
["DI-174","PB-CHB motor ORG fail alarm","腔体拨杆伺服M2找原点失败报警",null,"W20.14"]
["DI-175","PB-IN motor ORG fail alarm","进料推杆伺服M3找原点失败报警",null,"W20.15"]
["DI-176","LS-IN motor ABS fail alarm","进料升降伺服M0绝对定位失败报警",null,"W21.00"]
["DI-177","LS-OUT motor ABS fail alarm","出料升降伺服M1绝对定位失败报警",null,"W21.01"]
["DI-178","PB-CHB motor ABS fail alarm","腔体拨杆伺服M2绝对定位失败报警",null,"W21.02"]
["DI-179","PB-IN motor ABS fail alarm","进料推杆伺服M3绝对定位失败报警",null,"W21.03"]
["DI-180","BOX not placed well alarm","料盒未放置好异常报警",null,"W21.04"]
["DI-181","Replace the  box overtime alarm","换料盒超时异常报警",null,"W21.05"]
["DI-182","Replace the feeding box alarm","换料盒时进料口卡料异常报警",null,"W21.06"]
["DI-183","PB-IN sticking alarm","进料推杆卡住异常报警",null,"W21.07"]
["DI-184","PB-CHB sticking  alarm","腔体拨杆卡住异常报警",null,"W21.08"]
["DI-185","PB-OUT sticking  alarm","出料拨杆卡住异常报警",null,"W21.09"]
["DI-186","TS-IN entrance sticking  alarm","进料传送平台入口处卡料异常报警",null,"W21.10"]
["DI-187","TS-IN exit sticking  alarm","进料传送平台出口处卡料异常报警",null,"W21.11"]
["DI-188","TS-OUT entrance sticking  alarm","出料传送平台入口处卡料异常报警",null,"W21.12"]
["DI-189","TS-OUT exit sticking  alarm","出料传送平台出口处卡料异常报警",null,"W21.13"]
["DI-190","LS-OUT entrance sticking  alarm","出料升降平台入口处卡料异常报警",null,"W21.14"]
["DI-191","PB-CHB push out fail alarm","腔体推出料板失败报警",null,"W21.15"]
["DI-192","PB-CHB U&D cylinder down alarm","腔体拨杆上下气缸未下降到位报警",null,"W22.00"]
["DI-193","R-IN U&D cylinder up alarm","进料轨道止档气缸未上升到位报警",null,"W22.01"]
["DI-194","R-IN L&R cylinder R-Moving alarm","进料轨道平移气缸未右移到位报警",null,"W22.02"]
["DI-195","PB-OUT U&D cylinder down alarm","出料拨杆上下气缸未下降到位报警",null,"W22.03"]
["DI-196","PB-OUT F&B cylinder R-Moving alarm","出料拨杆推料气缸未右移到位报警",null,"W22.04"]
["DI-197","R-OUT U&D cylinder  up alarm","出料轨道止档气缸未上升到位报警",null,"W22.05"]
["DI-198","R-OUT L&R cylinder  R-Moving alarm","出料轨道平移气缸未右移到位报警",null,"W22.06"]
["DI-199",null,"备用",null,"W22.07"]
["DI-200","PB-CHB U&D cylinder up alarm","腔体拨杆上下气缸未上升到位报警",null,"W22.08"]
["DI-201","R-IN U&D cylinder down alarm","进料轨道止档气缸未下降到位报警",null,"W22.09"]
["DI-202","R-IN L&R cylinder L-Moving alarm","进料轨道平移气缸未左移到位报警",null,"W22.10"]
["DI-203","PB-OUT U&D cylinder up alarm","出料拨杆上下气缸未上升到位报警",null,"W22.11"]
["DI-204","PB-OUT F&B cylinder L-Moving alarm","出料拨杆推料气缸未左移到位报警",null,"W22.12"]
["DI-205","R-OUT U&D cylinder  down alarm","出料轨道止档气缸未下降到位报警",null,"W22.13"]
["DI-206","R-OUT L&R cylinder  L-Moving alarm","出料轨道平移气缸未左移到位报警",null,"W22.14"]
["DI-207",null,null,null,"W22.15"]
["DI-208","Manual model can not auto run","手动模式下无法自动运行",null,"W23.00"]
["DI-209","Alarming  can not auto run","异常报警中无法自动运行",null,"W23.01"]
["DI-210","EM stop can not manual and auto","紧急停止中无法切换到手动和自动模式",null,"W23.02"]
["DI-211","Auto runing can not Manual","自动运行中无法切换到手动模式",null,"W23.03"]
["DI-212","Communication failure with yaskawa alarm","和安川控制器通讯失败异常报警",null,"W23.04"]
["DI-213","Unconfirmed Cleared can not  auto run","初次未确认物料清除无法自动运行",null,"W23.05"]
["DI-214","Material not cleared alarm","物料未被清除报警",null,"W23.06"]
["DI-215","OMRON cpu battery alarm","欧姆龙CPU电池电压低",null,"W23.07"]
["DI-216","YASKAWA cpu battery alarm","安川控制器CPU电池电压低",null,"W23.08"]
["DI-217","recipe not  uploaded alarm","配方未上传异常报警",null,"W23.09"]
["DI-218","LS-IN motor lost origin alarm","M0进料升降伺服原点异常丢失报警",null,"W23.10"]
["DI-219","LS-OUT motor lost origin alarm","M1进料升降伺服原点异常丢失报警",null,"W23.11"]
["DI-220","PB-CHB motor lost origin alarm","M2进料升降伺服原点异常丢失报警",null,"W23.12"]
["DI-221","PB-IN motor lost origin alarm","M3进料升降伺服原点异常丢失报警",null,"W23.13"]
[{"$nulls":4},"W23.14"]
[null,"缩写","中文含义","英文含义"]
[null,"R1","轨道1","Rail 1"]
[null,"R2","轨道2","Rail 2"]
[null,"R3","轨道3","Rail 3"]
[null,"R4","轨道4","Rail 4"]
[null,"CHB","腔体","Chamber"]
[null,"F&B","前后","Front And Back"]
[null,"L&R","左右","Left And Right"]
[null,"LS","载料平台","Load Station"]
[null,"MGZ","料盒","magazine"]
[null,"R","轨道","Rail"]
[null,"PB","推杆","Push Bar"]
[null,"TS","交换平台","Transfer Station"]
[null,"U&D","上下","Up And Down"]
[null,"FB","返回值","Feedback"]
[]
[null,"缩写组合含义举例","中文含义","英文含义"]
[null,"LS_IN","进料平台","Load Station In"]
[null,"PB_CHB","腔体推杆","Push Bar Chamber"]
[null,"R1-OUT","出料轨道1","Rail 1 Out"]

{"sheet":"AO","index":2,"n_rows":81,"n_cols":9,"rows_kept":81,"cut":false,"hidden":false,"merged":[[63,8,69,8]]}
["Node No. ","ID","Range","Scale","Device Name","Logic note","date type","Note"]
["AO-00","d100",null,null,"M0 speed",null,"32Float","M0运行速度"]
["AO-01","d102",null,null,"M1 speed",null,"32Float","M1运行速度"]
["AO-02","d104",null,null,"M2 speed",null,"32Float","M2运行速度"]
["AO-03","d106",null,null,"M3 speed",null,"32Float","M3运行速度"]
["AO-04","d108",null,null,"M0 manual speed",null,"32Float","M0手动速度"]
["AO-05","d110",null,null,"M1 manual speed",null,"32Float","M1手动速度"]
["AO-06","d112",null,null,"M2 manual speed",null,"32Float","M2手动速度"]
["AO-07","d114",null,null,"M3 manual speed",null,"32Float","M3手动速度"]
["AO-08","d116",null,null,"M0 acceleration(single)",null,"32Float","M0加速比率(单字)"]
["AO-09","d118",null,null,"M0 deceleration(single)",null,"32Float","M0减速比率(单字)"]
["AO-10","d120",null,null,"M0 start frequency",null,"32Float","M0启动频率"]
["AO-11","d122",null,null,"M1 acceleration(single)",null,"32Float","M1加速比率(单字)"]
["AO-12","d124",null,null,"M1 deceleration(single)",null,"32Float","M1减速比率(单字)"]
["AO-13","d126",null,null,"M1 start frequency",null,"32Float","M1启动频率"]
["AO-14","d128",null,null,"M2 acceleration(single)",null,"32Float","M2加速比率(单字)"]
["AO-15","d130",null,null,"M2 deceleration(single)",null,"32Float","M2减速比率(单字)"]
["AO-16","d132",null,null,"M2 start frequency",null,"32Float","M2启动频率"]
["AO-17","d134",null,null,"M3 acceleration(single)",null,"32Float","M3加速比率(单字)"]
["AO-18","d136",null,null,"M3 deceleration(single)",null,"32Float","M3减速比率(单字)"]
["AO-19","d138",null,null,"M3 start frequency",null,"32Float","M3启动频率"]
["AO-20","d140",null,null,"M0 LS-IN MGZ location data",null,"32Float","M0定位位置"]
["AO-21","d142",null,null,"M1 LS-OUT MGZ location data",null,"32Float","M1定位位置"]
["AO-22","d144",null,null,"M2 PB-CHB location data",null,"32Float","M2定位位置"]
["AO-23","d146",null,null,"M3 PB-IN location data",null,"32Float","M3定位位置"]
["AO-24","d148",null,null,"LS-IN origin speed",null,"32 float","M0搜索原点速度(mm/s)"]
["AO-25","d150",null,null,"LS-OUT origin speed",null,"32 float","M1搜索原点速度"]
["AO-26","d152",null,null,"PB-CHB origin speed",null,"32 float","M2搜索原点速度"]
["AO-27","d154",null,null,"PB-IN origin speed",null,"32 float","M3搜索原点速度"]
["AO-28","d156",null,null,"LS-IN Acc/Dec time",null,"32 float","M0加减速时间参数(ms)"]
["AO-29","d158",null,null,"LS-OUT  Acc/Dec time",null,"32 float","M1加减速时间参数"]
["AO-30","d160",null,null,"PB-CHB Acc/Dec time",null,"32 float","M2加减速时间参数"]
["AO-31","d162",null,null,"PB-IN Acc/Dec time",null,"32 float","M3加减速时间参数"]
["AO-32","d164",null,null,"LS-IN CCW limit position",null,"32 float","M0伺服负极限位置（mm)"]
["AO-33","d166",null,null,"LS-OUT CCW limit position",null,"32 float","M1伺服负极限位置（mm)"]
["AO-34","d168",null,null,"PB-CHB CCW limit position",null,"32 float","M2伺服负极限位置（mm)"]
["AO-35","d170",null,null,"PB-IN CCW limit position",null,"32 float","M3伺服负极限位置（mm)"]
["AO-36","d172",null,null,"LS-IN CW limit position",null,"32 float","M0伺服正极限位置（mm)"]
["AO-37","d174",null,null,"LS-OUT CW limit position",null,"32 float","M1伺服正极限位置（mm)"]
["AO-38","d176",null,null,"PB-CHB CW limit position",null,"32 float","M2伺服正极限位置（mm)"]
["AO-39","d178",null,null,"PB-IN CW limit position",null,"32 float","M3伺服正极限位置（mm)"]
["AO-40","d180",null,null,"PB-CHB  no interference position",null,"32 float","M2伺服拨杆对腔体无干涉处（mm)"]
["AO-41","d182",null,null,"PB-IN no interference position",null,"32 float","M3伺服推杆对进料升降平台无干涉处（mm)"]
["AO-42","d184",{"$nulls":4},"32 float","备用"]
["AO-43","d186",{"$nulls":4},"32 float","备用"]
["AO-44","d188",{"$nulls":4},"32 float","备用"]
["AO-45","d190",{"$nulls":4},"32 float","备用"]
["AO-46","d192",null,null,"LS-IN target number of plies",null,"32 float","指定M0目标层数值"]
["AO-47","d194",null,null,"LS-OUT target number of plies",null,"32 float","指定M1目标层数值"]
["AO-48","d196",{"$nulls":4},"32 float","备用"]
["AO-49","d198",{"$nulls":4},"32 float","备用"]
["AO-50","d200",null,null,"U/D Cylinder arrival time",null,"32 float","上下气缸确认到位时间（S）"]
["AO-51","d202",null,null,"L/R Cylinder arrival time",null,"32 float","左右气缸确认到位时间"]
["AO-52","d204",null,null,"Box arrival time",null,"32 float","LS-in和LS-out区确认有料箱时间（S）"]
["AO-53","d206",null,null,"Material arrival time",null,"32 float","TS-in和TS-out区出口处料件确认到达时间"]
["AO-54","d208",null,null,"Entrance stick  time ",null,"32 float","TS-in和TS-out区确认入口处卡料报警时间（S）"]
["AO-55","d210",null,null,"Exit stick  time ",null,"32 float","TS-in和TS-out区确认出口处卡料报警时间"]
["AO-56","d212",{"$nulls":4},"32 float","备用"]
["AO-57","d214",{"$nulls":4},"32 float","备用"]
["AO-58","d216",{"$nulls":4},"32 float","备用"]
["AO-59","d218",{"$nulls":4},"32 float","备用"]
["AO-60","d220",{"$nulls":4},"32 float","备用"]
["AO-61","d222",null,null,"TM_Heartbeat",null,"32 float","心跳信号数值"]
["AO-62","d224",null,null,"Product number of plies",null,"32 float","产品总层数","配方"]
["AO-63","d226",null,null,"Product floor space",null,"32 float","每层间距（mm)"]
["AO-64","d228",null,null,"Product length",null,"32 float","产品长度（mm)"]
["AO-65","d230",null,null,"Product width",null,"32 float","产品宽度（mm)"]
["AO-66","d232",null,null,"LS-in  first floor position",null,"32 float","进料平台机种首层位置（mm)"]
["AO-67","d234",null,null,"LS-out  first floor position",null,"32 float","出料平台机种首层位置（mm)"]
["AO-68","d236",null,null,"Product margin",null,"32 float","产品离基准面距离（mm)"]
["AO-69","d238",null,null,"PB-CHB Motor push-in  place",null,"32 float","PB-CHB区M2拨杆推入腔体正中总位置（mm)"]
["AO-70","d240",null,null,"PB-CHB Motor push-out  place",null,"32 float","PB-CHB区M2拨杆推出处总位置（mm)"]
["AO-71","d242",null,null,"LS-IN Motor work place",null,"32 float","LS-in区M3推杆推出处总位置（mm)"]
["AO-72","d244",null,null,"LS-IN Motor Initial place",null,"32 float","LS-in区M3推杆初始处（mm)"]
["AO-73","d246",null,null,"PB-CHB Motor Initial place",null,"32 float","PB-CHB区M2拨杆初始处（mm)"]
["AO-74","d248",null,null,"LS-IN motor Correction value",null,"32 float","M0伺服校准值"]
["AO-75","d250",null,null,"LS-OUT motor Correction value",null,"32 float","M1伺服校准值"]
["AO-76","d252",null,null,"PB-CHB  motor Correction value",null,"32 float","M2伺服校准值"]
["AO-77","d254",null,null,"PB-IN  motor Correction value",null,"32 float","M3伺服校准值"]
["AO-78","d256",null,null,"TM_Origin times",null,"32 float","重新回原点设备换料盒次数"]
["AO-79","d258",null,null,"Replace the feeding box place",null,"32 float","更换进料盒M0位置"]

{"sheet":"AI","index":3,"n_rows":53,"n_cols":8,"rows_kept":53,"cut":false,"hidden":false,"merged":[]}
["Node No. ","ID","Range","Scale","Device Name","Logic note","date type","Note"]
["AI-00","d300",null,null,"LS-IN motor M0 pulse current value",null,"32Float","M0当前绝对位置"]
["AI-01","d302",null,null,"LS-OUT motor M1 pulse current value",null,"32Flaot","M1当前绝对位置"]
["AI-02","d304",null,null,"PB-CHB motor M2 pulse current value",null,"32Float","M2当前绝对位置"]
["AI-03","d306",null,null,"PB-IN motor M3 pulse current value",null,"32Flaot","M3当前绝对位置"]
["AI-04","d308",null,null,"M0 speed FB",null,"32Float","M0运行速度返回值"]
["AI-05","d310",null,null,"M1 speed FB",null,"32Flaot","M1运行速度返回值"]
["AI-06","d312",null,null,"M2 speed FB",null,"32Float","M2运行速度返回值"]
["AI-07","d314",null,null,"M3 speed FB",null,"32Flaot","M3运行速度返回值"]
["AI-08","d316",null,null,"M0 manual speed FB",null,"32Float","M0手动速度返回值"]
["AI-09","d318",null,null,"M1 manual speed FB",null,"32Flaot","M1手动速度返回值"]
["AI-10","d320",null,null,"M2 manual speed FB",null,"32Float","M2手动速度返回值"]
["AI-11","d322",null,null,"M3 manual speed FB",null,"32Flaot","M3手动速度返回值"]
["AI-12","d324",null,null,"M0 acceleration(single) FB",null,"32Float","M0加速比率(单字)返回值"]
["AI-13","d326",null,null,"M0 deceleration(single) FB",null,"32Flaot","M0减速比率(单字)返回值"]
["AI-14","d328",null,null,"M0 start frequency FB",null,"32Float","M0启动频率返回值"]
["AI-15","d330",null,null,"M1 acceleration(single) FB",null,"32Flaot","M1加速比率(单字)返回值"]
["AI-16","d332",null,null,"M1 deceleration(single) FB",null,"32Float","M1减速比率(单字)返回值"]
["AI-17","d334",null,null,"M1 start frequency FB",null,"32Flaot","M1启动频率返回值"]
["AI-18","d336",null,null,"M2 acceleration(single) FB",null,"32Float","M2加速比率(单字)返回值"]
["AI-19","d338",null,null,"M2 deceleration(single) FB",null,"32Flaot","M2减速比率(单字)返回值"]
["AI-20","d340",null,null,"M2 start frequency FB",null,"32Float","M2启动频率返回值"]
["AI-21","d342",null,null,"M3 acceleration(single) FB",null,"32Flaot","M3加速比率(单字)返回值"]
["AI-22","d344",null,null,"M3 deceleration(single) FB",null,"32Float","M3减速比率(单字)返回值"]
["AI-23","d346",null,null,"M3 start frequency FB",null,"32Flaot","M3启动频率返回值"]
["AI-24","d348",null,null,"M0 LS-IN MGZ location data FB",null,"32Float","M0进料盒位置参数返回值"]
["AI-25","d350",null,null,"M1 LS-OUT MGZ location data FB",null,"32Flaot","M1出料盒位置参数返回值"]
["AI-26","d352",null,null,"M2 PB-CHB location data FB",null,"32Float","M2进料拨杆位置参数返回值"]
["AI-27","d354",null,null,"M3 PB-IN location data FB",null,"32Flaot","M3进料推杆位置参数返回值"]
["AI-28","d356",null,null,"LS-IN Servo  command  position",null,"32Float","M0当前指令位置"]
["AI-29","d358",null,null,"LS-OUT Servo  command  position",null,"32Flaot","M1当前指令位置"]
["AI-30","d360",null,null,"PB-CHB Servo  command  position",null,"32Float","M2当前指令位置"]
["AI-31","d362",null,null,"PB-IN Servo  command  position",null,"32Flaot","M3当前指令位置"]
["AI-32","d364",null,null,"LS-IN Servo Warning Code",null,"32Float","M0伺服Warning代码"]
["AI-33","d366",null,null,"LS-OUT Servo Warning Code",null,"32Flaot","M1伺服Warning代码"]
["AI-34","d368",null,null,"PB-CHB Servo Warning Code",null,"32Float","M2伺服Warning代码"]
["AI-35","d370",null,null,"PB-IN Servo Warning Code",null,"32Flaot","M3伺服Warning代码"]
["AI-36","d372",null,null,"LS-IN Servo Alarm Code",null,"32Float","M0伺服Alarm代码"]
["AI-37","d374",null,null,"LS-OUT Servo Alarm Code",null,"32Flaot","M1伺服Alarm代码"]
["AI-38","d376",null,null,"PB-CHB Servo Alarm Code",null,"32Float","M2伺服Alarm代码"]
["AI-39","d378",null,null,"PB-IN Servo Alarm Code",null,"32Flaot","M3伺服Alarm代码"]
["AI-40","d380",null,null,"LS-IN Station State value",null,"32Float","LS-in 区运行状态值"]
["AI-41","d382",null,null,"TS-IN Station State value",null,"32Flaot","TS-in 区运行状态值"]
["AI-42","d384",null,null,"PB-CHB Station State value",null,"32Float","PB-CHB区运行状态值"]
["AI-43","d386",null,null,"TS-out  Station State value",null,"32Flaot","TS-out区运行状态值"]
["AI-44","d388",null,null,"LS-out  Station State value",null,"32Float","LS-out区运行状态值"]
["AI-45","d390",null,null,"LS-IN Station number of plies",null,"32Flaot","LS- in升降平台目标加工层数"]
["AI-46","d392",null,null,"LS-OUT Station number of plies",null,"32Float","LS- out升降平台目标加工层数"]
["AI-47","d394",{"$nulls":4},"32Flaot","备用"]
["AI-48","d396",{"$nulls":4},"32Float","备用"]
["AI-49","d398",{"$nulls":4},"32Flaot","备用"]
["AI-50","d400",{"$nulls":4},"32Float","备用"]
["AI-51","d402",null,null,"TM_Heartbeat fb",null,"32Flaot","心跳信号数值（反馈值）"]