{"text_format":"2","workbook":"xlsx","n_sheets":4,"sheets":["Sheet1","DI-DO","AO","AI"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":4,"n_cols":4,"rows_kept":4,"cut":false,"hidden":false,"merged":[]}
[null,null,null,"PLC TO PC ==AI"]
[null,null,null,"PC TO PLC ==AO"]
[null,null,null,"DI== PLC TO PC"]
[null,null,null,"DO== PC TO PLC"]

{"sheet":"DI-DO","index":1,"n_rows":121,"n_cols":15,"rows_kept":121,"cut":false,"hidden":false,"merged":[]}
["DI","Name","Note","Postion (NO Power)","Location","Logic Note",null,null,"#.DO","ID","Name","EV No.","Note","Location","Logic Note"]
["DI-00","Signal_LS-IN motor origin","M0进料升降马达原点信号",null,"W0.00","1==on ,0==off",null,null,"DO-00",null,"Brake relay_LS-IN",null,"进料升降台刹车继电器","W10.00","1== 松开,0== 刹住"]
["DI-01","Signal_LS-IN motor CW limit ","M0进料升降马达CW限位信号",null,"W0.01","1==normal ,0== error",null,null,"DO-01",null,"Brake relay_LS-OUT",null,"出料升降台刹车继电器","W10.01","1== 松开,0== 刹住"]
["DI-02","Signal_LS-IN motor CCW limit ","M0进料升降马达CCW限位信号",null,"W0.02","1==normal ,0== error",null,null,"DO-02",null,"Motor M0 ON_LS-IN",null,"进料升降台马达M0伺服ON","W10.02","1== on,0== off"]
["DI-03","Signal_LS-OUT motor origin","M1出料升降马达原点信号",null,"W0.03","1==on ,0== off",null,null,"DO-03",null,"Motor M1 ON_LS-OUT",null,"出料升降台马达M1伺服ON","W10.03","1== on,0== off"]
["DI-04","Signal_LS-OUT motor CW limit ","M1出料升降马达CW限位信号",null,"W0.04","1==normal ,0== error",null,null,"DO-04",null,"Motor M2 ON_PB-CHB",null,"进料拨杆马达M2伺服ON","W10.04","1== on,0== off"]
["DI-05","Signal_LS-OUT motor CCW limit ","M1出料升降马达CCW限位信号",null,"W0.05","1==normal ,0== error",null,null,"DO-05",null,"Motor M3 ON_PB-IN",null,"进料推杆马达M3伺服ON","W10.05","1== on,0== off"]
["DI-06","Signal_PB-CHB origin","M2进料拨杆马达原点信号",null,"W0.06","1==on ,0==off",null,null,"DO-06",{"$nulls":4},"W10.06"]
["DI-07","Sensor_PB-CHB CW limit ","M2进料拨杆CW限位传感器",null,"W0.07","1==normal ,0== error",null,null,"DO-07",null,"PB-CHB U&D cylinder",null,"进料拨杆上下气缸","W10.07","1== 下,0==上"]
["DI-08","Sensor_PB-CHB CCW limit ","M2进料拨杆CCW限位传感器",null,"W0.08","1==normal ,0== error",null,null,"DO-08",null,"R-IN U&D cylinder",null,"进料轨道止档气缸","W10.08","1== 上,0== 下"]
["DI-09","Signal_PB-IN origin","M3进料推杆马达原点信号",null,"W0.09","1==on,0== off",null,null,"DO-09",null,"R-IN L&R cylinder",null,"进料轨道左右平移气缸","W10.09","1== 右,0==左"]
["DI-10","Sensor_PB-IN CW limit ","M3进料推杆CW限位传感器",null,"W0.10","1==normal ,0== error",null,null,"DO-10",null,"R-IN motor relay",null,"进料轨道马达继电器","W10.10","1==on,0==off"]
["DI-11","Sensor_PB-IN CCW limit ","M3进料推杆CCW限位传感器",null,"W0.11","1==normal ,0== error",null,null,"DO-11",null,"PB-OUT U&D cylinder",null,"出料拨杆上下气缸","W10.11","1== 下,0==上"]
["DI-12","Signal_LS-IN locating complete","进料升降马达驱动器定位完成信号(驱动器)",null,"W0.12","1==ok ,0== no",null,null,"DO-12",null,"PB-OUT F&B cylinder",null,"出料拨杆前后气缸","W10.12","0==左,1==右"]
["DI-13","Signal_LS-IN alarm ","进料升降马达驱动器报警信号(驱动器)",null,"W0.13","1==normal ,0== error",null,null,"DO-13",null,"R-OUT U&D cylinder",null,"出料轨道止档气缸","W10.13","1== 上,0== 下"]
["DI-14","Signal_LS-OUT locating complete","出料升降马达驱动器定位完成信号(驱动器)",null,"W0.14","1==ok ,0== no",null,null,"DO-14",null,"R-OUT L&R cylinder",null,"出料轨道左右平移气缸","W10.14","1== 右,0==左"]
["DI-15","Signal_LS-OUT alarm ","出料升降马达驱动器报警信号(驱动器)",null,"W0.15","1==normal ,0== error",null,null,"DO-15",null,"R-OUT motor relay",null,"出料轨道马达继电器","W10.15","1==on,0==off"]
["DI-16","Signal_PB-CHB locating complete","进料拨杆马达驱动器定位完成信号(驱动器)",null,"W1.00","1==ok ,0== no",null,null,"DO-16",null,"LS-IN M0 manual operate rising",null,"进料升降台M0手动上升","W11.00","1==on,0==off"]
["DI-17","Signal_PB-CHB alarm ","进料拨杆马达驱动器报警信号(驱动器)",null,"W1.01","1==normal ,0== error",null,null,"DO-17",null,"LS-IN M0 manual operate declining",null,"进料升降台M0手动下降","W11.01","1==on,0==off"]
["DI-18","Signal_PB-IN locating complete","进料推杆马达驱动器定位完成信号(驱动器)",null,"W1.02","1==ok ,0== no",null,null,"DO-18",null,"LS-OUT M1 manual operate rising",null,"出料升降台M1手动上升","W11.02","1==on,0==off"]
["DI-19","Signal_PB-IN alarm ","进料推杆马达驱动器报警信号(驱动器)",null,"W1.03","1==normal ,0== error",null,null,"DO-19",null,"LS-OUT M1 manual operate declining",null,"出料升降台M1手动下降","W11.03","1==on,0==off"]
["DI-20","Sensor_PB-IN prevent sticking","进料推杆防卡传感器",null,"W1.04","0==normal ,1== error",null,null,"DO-20",null,"PB-CHB M2 manual operate moving left",null,"进料拨杆M2手动向左","W11.04","1==on,0==off"]
["DI-21","Sensor_PB-CHB prevent sticking","进料拨杆防卡传感器",null,"W1.05","0==normal ,1== error",null,null,"DO-21",null,"PB-CHB M2 manual operate moving right",null,"进料拨杆M2手动向右","W11.05","1==on,0==off"]
["DI-22","Sensor_PB-OUT prevent sticking","出料拨杆防卡传感器",null,"W1.06","0==normal ,1== error",null,null,"DO-22",null,"PB-IN M3 manual operate moving left",null,"进料推杆M3手动向左","W11.06","1==on,0==off"]
["DI-23","Sensor_R4-IN entrance","进料前轨道入口传感器",null,"W1.07","1==on ,0== off",null,null,"DO-23",null,"PB-IN M3 manual operate moving right",null,"进料推杆M3手动向右","W11.07","1==on,0==off"]
["DI-24","Sensor_R4-IN stop bit","进料前轨道停止位传感器",null,"W1.08","1==on ,0== off",null,null,"DO-24",null,"LS-IN MGZ go to M0 location",null,"去M0进料盒指定位置","W11.08","1==on,0==off"]
["DI-25","Sensor_R3-IN entrance","进料中前轨道入口传感器",null,"W1.09","1==on ,0== off",null,null,"DO-25",null,"LS-OUT MGZ go to M1 location",null,"去M1出料盒指定位置","W11.09","1==on,0==off"]
["DI-26","Sensor_R3-IN stop bit","进料中前轨道停止位传感器",null,"W1.10","1==on ,0== off",null,null,"DO-26",null,"PB-CHB go to M2 location",null,"去M2进料拨杆指定位置","W11.10","1==on,0==off"]
["DI-27","Sensor_R2-IN entrance","进料中后轨道入口传感器",null,"W1.11","1==on ,0== off",null,null,"DO-27",null,"PB-IN go to M3 location",null,"去M3进料推杆指定位置","W11.11","1==on,0==off"]
["DI-28","Sensor_R2-IN stop bit","进料中后轨道停止位传感器",null,"W1.12","1==on ,0== off",null,null,"DO-28",null,"M0 deviation counter reset",null,"M0偏差计数器复位","W11.12","1==on,0==off"]
["DI-29","Sensor_R1-IN entrance","进料后轨道入口传感器",null,"W1.13","1==on ,0== off",null,null,"DO-29",null,"M1 deviation counter reset",null,"M1偏差计数器复位","W11.13","1==on,0==off"]
["DI-30","Sensor_R1-IN stop bit","进料后轨道停止位传感器",null,"W1.14","1==on ,0== off",null,null,"DO-30",null,"M2 deviation counter reset",null,"M2偏差计数器复位","W11.14","1==on,0==off"]
["DI-31","Sensor_PB-CHB U&D cylinder A top ","进料拨杆上下气缸A上位传感器",null,"W1.15","1==on ,0== off",null,null,"DO-31",null,"M3 deviation counter reset",null,"M3偏差计数器复位","W11.15","1==on,0==off"]
["DI-32","Sensor_PB-CHB U&D cylinder A bottom ","进料拨杆上下气缸A下位传感器",null,"W2.00","1==on ,0== off",null,null,"DO-32",null,"M0 Driver alarm reset",null,"M0驱动器报警复位","W12.00","1== en,0== close"]
["DI-33","Sensor_R-IN L&R cylinder left ","进料轨道左右平移气缸左位传感器",null,"W2.01","1==on ,0== off",null,null,"DO-33",null,"M1 Driver alarm reset",null,"M1驱动器报警复位","W12.01","1== en,0== close"]
["DI-34","Sensor_R-IN L&R cylinder right ","进料轨道左右平移气缸右位传感器",null,"W2.02","1==on ,0== off",null,null,"DO-34",null,"M2 Driver alarm reset",null,"M2驱动器报警复位","W12.02","1== en,0== close"]
["DI-35","Sensor_R-IN U&D cylinder top ","进料轨道止档气缸上位传感器",null,"W2.03","1==on ,0== off",null,null,"DO-35",null,"M3 Driver alarm reset",null,"M3驱动器报警复位","W12.03","1== en,0== close"]
["DI-36","Sensor_R-IN U&D cylinder bottom ","进料轨道止档气缸下位传感器",null,"W2.04","1==on ,0== off",null,null,"DO-36",null,"M0 manual operate stop rising ",null,"M0手动上升停止","w12.04","1== en,0== close"]
["DI-37","Sensor_LS-IN MGZ4","进料前料盒检测传感器",null,"W2.05","1==on ,0== off",null,null,"DO-37",null,"M0 manual operate stop declining",null,"M0手动下降停止","w12.05","1== en,0== close"]
["DI-38","Sensor_LS-IN MGZ3","进料中前料盒检测传感器",null,"W2.06","1==on ,0== off",null,null,"DO-38",null,"M1 manual operate stop rising",null,"M1手动上升停止","w12.06","1== en,0== close"]
["DI-39","Sensor_LS-IN MGZ2","进料中后料盒检测传感器",null,"W2.07","1==on ,0== off",null,null,"DO-39",null,"M1 manual operate stop declining",null,"M1手动下降停止","w12.07","1== en,0== close"]
["DI-40","Sensor_LS-IN MGZ1","进料后料盒检测传感器",null,"W2.08","1==on ,0== off",null,null,"DO-40",null,"M2 manual operate stop moving left",null,"M2手动向左停止","w12.08","1== en,0== close"]
["DI-41","Sensor_R4-OUT entrance","出料前轨道入口传感器",null,"W2.09","1==on ,0== off",null,null,"DO-41",null,"M2 manual operate stop moving right",null,"M2手动向右停止","w12.09","1== en,0== close"]
["DI-42","Sensor_R4-OUT stop bit","出料前轨道停止位传感器",null,"W2.10","1==on ,0== off",null,null,"DO-42",null,"M3 manual operate stop moving left",null,"M3手动向左停止","w12.10","1== en,0== close"]
["DI-43","Sensor_R4-OUT exit","出料前轨道出口传感器",null,"W2.11","1==on ,0== off",null,null,"DO-43",null,"M3 manual operate stop moving right",null,"M3手动向右停止","w12.11","1== en,0== close"]
["DI-44","Sensor_R3-OUT entrance","出料中前轨道入口传感器",null,"W2.12","1==on ,0== off",null,null,"DO-44",null,"M0 looking for origin",null,"M0搜索原点","w12.12","1== en,0== close"]
["DI-45","Sensor_R3-OUT stop bit","出料中前轨道停止位传感器",null,"W2.13","1==on ,0== off",null,null,"DO-45",null,"M1 looking for origin",null,"M1搜索原点","w12.13","1== en,0== close"]
["DI-46","Sensor_R3-OUT exit","出料中前轨道出口传感器",null,"W2.14","1==on ,0== off",null,null,"DO-46",null,"M2 looking for origin",null,"M2搜索原点","w12.14","1== en,0== close"]
["DI-47","Sensor_R2-OUT entrance","出料中后轨道入口传感器",null,"W2.15","1==on ,0== off",null,null,"DO-47",null,"M3 looking for origin",null,"M3搜索原点","w12.15","1== en,0== close"]
["DI-48","Sensor_R2-OUT stop bit","出料中后轨道停止位传感器",null,"W3.00","1==on ,0== off",null,null,"DO-48",null,"Init",null,"系统复位","w13.00","1== en,0== close"]
["DI-49","Sensor_R2-OUT exit","出料中后轨道出口传感器",null,"W3.01","1==on ,0== off",null,null,"DO-49",null,"reset（PC）",null,"故障清除","w13.01","1== en,0== close"]
["DI-50","Sensor_R1-OUT entrance","出料后轨道入口传感器",null,"W3.02","1==on ,0== off",null,null,"DO-50",null,"Load Station In Clear Error",null,"进料升降台故障清除","w13.02","1==on,0==off"]
["DI-51","Sensor_R1-OUT stop bit","出料后轨道停止位传感器",null,"W3.03","1==on ,0== off",null,null,"DO-51",null,"PM Clear Error",null,"进料拨杆故障清除","w13.03","1==on,0==off"]
["DI-52","Sensor_R1-OUT exit","出料后轨道出口传感器",null,"W3.04","1==on ,0== off",null,null,"DO-52",null,"Load Station Out Clear Error",null,"出料升降台故障清除","w13.04","1==on,0==off"]
["DI-53","Sensor_PB-OUT U&D cylinder A top ","出料拨杆上下气缸A上位传感器",null,"W3.05","1==on ,0== off"]
["DI-54","Sensor_PB-OUT U&D cylinder A bottom ","出料拨杆上下气缸A下位传感器",null,"W3.06","1==on ,0== off"]
["DI-55","Sensor_PB-OUT L&R cylinder left ","出料拨杆左右气缸左位传感器",null,"W3.07","1==on ,0== off"]
["DI-56","Sensor_PB-OUT L&R cylinder right ","出料拨杆左右气缸右位传感器",null,"W3.08","1==on ,0== off"]
["DI-57","Sensor_R-OUT L&R cylinder left ","出料轨道左右平移气缸左位传感器",null,"W3.09","1==on ,0== off"]
["DI-58","Sensor_R-OUT L&R cylinder right ","出料轨道左右平移气缸右位传感器",null,"W3.10","1==on ,0== off"]
["DI-59","Sensor_R-OUT U&D cylinder top ","出料止档气缸上位传感器",null,"W3.11","1==on ,0== off"]
["DI-60","Sensor_R-OUT U&D cylinder bottom ","出料止档气缸下位传感器",null,"W3.12","1==on ,0== off"]
["DI-61","Sensor_LS-OUT MGZ4","出料前料盒检测传感器",null,"W3.13","1==on ,0== off"]
["DI-62","Sensor_LS-OUT MGZ3","出料中前料盒检测传感器",null,"W3.14","1==on ,0== off"]
["DI-63","Sensor_LS-OUT MGZ2","出料中后料盒检测传感器",null,"W3.15","1==on ,0== off"]
["DI-64","Sensor_LS-OUT MGZ1","出料后料盒检测传感器",null,"W4.00","1==on ,0== off"]
["DI-65","Sign_LS-IN motor M0 pulse output complete","进料升降马达M0脉冲输出完成标志(PLC信号)",null,"W4.01","1==ok ,0== no"]
["DI-66","Sign_LS-OUT motor M1 pulse output complete","出料升降马达M1脉冲输出完成标志(PLC信号)",null,"W4.02","1==ok ,0== no"]
["DI-67","Sign_PB-CHB motor M2 pulse output complete","进料拨杆马达M2脉冲输出完成标志(PLC信号)",null,"W4.03","1==ok ,0== no"]
["DI-68","Sign_PB-IN motor M3 pulse output complete","进料推杆马达M3脉冲输出完成标志(PLC信号)",null,"W4.04","1==ok ,0== no"]
["DI-69","Sign_LS-IN motor outputting M0 pulse ","进料升降马达M0脉冲输出中标志(PLC信号)",null,"W4.05","1==on ,0== off"]
["DI-70","Sign_LS-OUT motor outputting M1 pulse ","出料升降马达M1脉冲输出中标志(PLC信号)",null,"W4.06","1==on ,0== off"]
["DI-71","Sign_PB-CHB motor outputting M2 pulse ","进料拨杆马达M2脉冲输出中标志(PLC信号)",null,"W4.07","1==on ,0== off"]
["DI-72","Sign_PB-IN motor outputting M3 pulse ","进料推杆马达M3脉冲输出中标志(PLC信号)",null,"W4.08","1==on ,0== off"]
["DI-73","Sign_LS-IN motor M0 without origin","进料升降马达M0无原点标志(PLC信号)",null,"W4.09","1==无原点 ,0== ok"]
["DI-74","Sign_LS-OUT motor M1 without origin","出料升降马达M1无原点标志(PLC信号)",null,"W4.10","1==无原点 ,0== ok"]
["DI-75","Sign_PB-CHB motor M2 without origin","进料拨杆马达M2无原点标志(PLC信号)",null,"W4.11","1==无原点 ,0== ok"]
["DI-76","Sign_PB-IN motor M3 without origin ","进料推杆马达M3无原点标志(PLC信号)",null,"W4.12","1==无原点 ,0== ok"]
["DI-77","Sign_LS-IN motor M0 locating complete","进料升降马达M0定位完成标志(PLC信号)",null,"W4.13","1==ok ,0== no"]
["DI-78","Sign_LS-OUT motor M1 locating complete","出料升降马达M1定位完成标志(PLC信号)",null,"W4.14","1==ok ,0== no"]
["DI-79","Sign_PB-CHB motor M2 locating complete","进料拨杆马达M2定位完成标志(PLC信号)",null,"W4.15","1==ok ,0== no"]
["DI-80","Sign_PB-IN motor M3 locating complete","进料推杆马达M3定位完成标志(PLC信号)",null,"W5.00","1==ok ,0== no"]
["DI-81","EMO","急停信号",null,"W5.01"]
["DI-82","Safe Interlock","安全门",null,"W5.02"]
["DI-83",null,null,null,"W5.03"]
["DI-84",null,null,null,"W5.04"]
["DI-85","Sensor_PB-CHB U&D cylinder B top ","进料拨杆上下气缸B上位传感器",null,"W5.05","1==on ,0== off"]
["DI-86","Sensor_PB-CHB U&D cylinder B bottom ","进料拨杆上下气缸B下位传感器",null,"W5.06","1==on ,0== off"]
["DI-87","Sensor_PB-OUT U&D cylinder B top ","出料拨杆上下气缸B上位传感器",null,"W5.07","1==on ,0== off"]
["DI-88","Sensor_PB-OUT U&D cylinder B bottom ","出料拨杆上下气缸B下位传感器",null,"W5.08","1==on ,0== off"]
["DI-89","Init Completed","系统复位完成标志",null,"W5.09","1==ok ,0== no"]
["DI-90","Motor M0 ON_LS-IN FB","进料升降台马达M0伺服ON标志",null,"W5.10","1==ok ,0== no"]
["DI-91","Motor M1 ON_LS-OUT FB","出料升降台马达M1伺服ON标志",null,"W5.11","1==ok ,0== no"]
["DI-92","Motor M2 ON_PB-CHB FB","进料拨杆马达M2伺服ON标志",null,"W5.12","1==ok ,0== no"]
["DI-93","Motor M3 ON_PB-IN FB","进料推杆马达M3伺服ON标志",null,"W5.13","1==ok ,0== no"]
[]
[]
[]
[]
[]
[]
[null,"缩写","中文含义","英文含义"]
[null,"R1","轨道1","Rail 1"]
[null,"R2","轨道2","Rail 2"]
[null,"R3","轨道3","Rail 3"]
[null,"R4","轨道4","Rail 4"]
[null,"CHB","腔体","Chamber"]
[null,"F&B","前后","Front And Back"]
[null,"L&R","左右","Left And Right"]
[null,"LS","载料平台","Load Station"]
[null,"MGZ","料盒","magazine"]
[null,"R","轨道","Rail"]
[null,"PB","推杆","Push Bar"]
[null,"TS","交换平台","Transfer Station"]
[null,"U&D","上下","Up And Down"]
[null,"FB","返回值","Feedback"]
[]
[null,"缩写组合含义举例","中文含义","英文含义"]
[null,"LS_IN","进料平台","Load Station In"]
[null,"PB_CHB","腔体推杆","Push Bar Chamber"]
[null,"R1-OUT","出料轨道1","Rail 1 Out"]

{"sheet":"AO","index":2,"n_rows":25,"n_cols":8,"rows_kept":25,"cut":false,"hidden":false,"merged":[]}
["Node No. ","ID","Range","Scale","Device Name","Logic note","date type","Note"]
["AO-00","d100",null,null,"M0 speed",null,"32HEX","M0运行速度"]
["AO-01","d102",null,null,"M1 speed",null,"32HEX","M1运行速度"]
["AO-02","d104",null,null,"M2 speed",null,"32HEX","M2运行速度"]
["AO-03","d106",null,null,"M3 speed",null,"32HEX","M3运行速度"]
["AO-04","d108",null,null,"M0 manual speed",null,"32HEX","M0手动速度"]
["AO-05","d110",null,null,"M1 manual speed",null,"32HEX","M1手动速度"]
["AO-06","d112",null,null,"M2 manual speed",null,"32HEX","M2手动速度"]
["AO-07","d114",null,null,"M3 manual speed",null,"32HEX","M3手动速度"]
["AO-08","d116",null,null,"M0 acceleration(single)",null,"32HEX","M0加速比率(单字)"]
["AO-09","d118",null,null,"M0 deceleration(single)",null,"32HEX","M0减速比率(单字)"]
["AO-10","d120",null,null,"M0 start frequency",null,"32HEX","M0启动频率"]
["AO-11","d122",null,null,"M1 acceleration(single)",null,"32HEX","M1加速比率(单字)"]
["AO-12","d124",null,null,"M1 deceleration(single)",null,"32HEX","M1减速比率(单字)"]
["AO-13","d126",null,null,"M1 start frequency",null,"32HEX","M1启动频率"]
["AO-14","d128",null,null,"M2 acceleration(single)",null,"32HEX","M2加速比率(单字)"]
["AO-15","d130",null,null,"M2 deceleration(single)",null,"32HEX","M2减速比率(单字)"]
["AO-16","d132",null,null,"M2 start frequency",null,"32HEX","M2启动频率"]
["AO-17","d134",null,null,"M3 acceleration(single)",null,"32HEX","M3加速比率(单字)"]
["AO-18","d136",null,null,"M3 deceleration(single)",null,"32HEX","M3减速比率(单字)"]
["AO-19","d138",null,null,"M3 start frequency",null,"32HEX","M3启动频率"]
["AO-20","d140",null,null,"M0 LS-IN MGZ location data",null,"32HEX","M0进料盒位置参数"]
["AO-21","d142",null,null,"M1 LS-OUT MGZ location data",null,"32HEX","M1出料盒位置参数"]
["AO-22","d144",null,null,"M2 PB-CHB location data",null,"32HEX","M2进料拨杆位置参数"]
["AO-23","d146",null,null,"M3 PB-IN location data",null,"32HEX","M3进料推杆位置参数"]

{"sheet":"AI","index":3,"n_rows":29,"n_cols":8,"rows_kept":29,"cut":false,"hidden":false,"merged":[]}
["Node No. ","ID","Range","Scale","Device Name","Logic note","date type","Note"]
["AI-00","d300",null,null,"LS-IN motor M0 pulse current value",null,"32HEX","进料升降马达M0脉冲输出当前值(PLC数据非驱动器)"]
["AI-01","d302",null,null,"LS-OUT motor M1 pulse current value",null,"32HEX","出料升降马达M1脉冲输出当前值(PLC数据非驱动器)"]
["AI-02","d304",null,null,"PB-CHB motor M2 pulse current value",null,"32HEX","进料拨杆马达M2脉冲输出当前值(PLC数据非驱动器)"]
["AI-03","d306",null,null,"PB-IN motor M3 pulse current value",null,"32HEX","进料推杆马达M3脉冲输出当前值(PLC数据非驱动器)"]
["AI-04","d308",null,null,"M0 speed FB",null,"32HEX","M0运行速度返回值"]
["AI-05","d310",null,null,"M1 speed FB",null,"32HEX","M1运行速度返回值"]
["AI-06","d312",null,null,"M2 speed FB",null,"32HEX","M2运行速度返回值"]
["AI-07","d314",null,null,"M3 speed FB",null,"32HEX","M3运行速度返回值"]
["AI-08","d316",null,null,"M0 manual speed FB",null,"32HEX","M0手动速度返回值"]
["AI-09","d318",null,null,"M1 manual speed FB",null,"32HEX","M1手动速度返回值"]
["AI-10","d320",null,null,"M2 manual speed FB",null,"32HEX","M2手动速度返回值"]
["AI-11","d322",null,null,"M3 manual speed FB",null,"32HEX","M3手动速度返回值"]
["AI-12","d324",null,null,"M0 acceleration(single) FB",null,"32HEX","M0加速比率(单字)返回值"]
["AI-13","d326",null,null,"M0 deceleration(single) FB",null,"32HEX","M0减速比率(单字)返回值"]
["AI-14","d328",null,null,"M0 start frequency FB",null,"32HEX","M0启动频率返回值"]
["AI-15","d330",null,null,"M1 acceleration(single) FB",null,"32HEX","M1加速比率(单字)返回值"]
["AI-16","d332",null,null,"M1 deceleration(single) FB",null,"32HEX","M1减速比率(单字)返回值"]
["AI-17","d334",null,null,"M1 start frequency FB",null,"32HEX","M1启动频率返回值"]
["AI-18","d336",null,null,"M2 acceleration(single) FB",null,"32HEX","M2加速比率(单字)返回值"]
["AI-19","d338",null,null,"M2 deceleration(single) FB",null,"32HEX","M2减速比率(单字)返回值"]
["AI-20","d340",null,null,"M2 start frequency FB",null,"32HEX","M2启动频率返回值"]
["AI-21","d342",null,null,"M3 acceleration(single) FB",null,"32HEX","M3加速比率(单字)返回值"]
["AI-22","d344",null,null,"M3 deceleration(single) FB",null,"32HEX","M3减速比率(单字)返回值"]
["AI-23","d346",null,null,"M3 start frequency FB",null,"32HEX","M3启动频率返回值"]
["AI-24","d348",null,null,"M0 LS-IN MGZ location data FB",null,"32HEX","M0进料盒位置参数返回值"]
["AI-25","d350",null,null,"M1 LS-OUT MGZ location data FB",null,"32HEX","M1出料盒位置参数返回值"]
["AI-26","d352",null,null,"M2 PB-CHB location data FB",null,"32HEX","M2进料拨杆位置参数返回值"]
["AI-27","d354",null,null,"M3 PB-IN location data FB",null,"32HEX","M3进料推杆位置参数返回值"]