{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Saturn Plus设备现场安装报告"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Saturn Plus设备现场安装报告","index":0,"n_rows":8,"n_cols":5,"rows_kept":8,"cut":false,"hidden":false,"merged":[[0,0,0,4],[1,0,1,4],[3,1,3,2],[5,0,5,4],[7,0,7,4],[2,1,2,4],[6,0,6,4],[4,0,4,4]]}
["上海稷以科技有限公司\nSHANGHAI JETPLASMA CO.,LTD\n上海市闵行区莲花南路2899号5号楼\nNo.2899 Lianlua Road, Shanghai, China\nTel：021-34125995   Web：www.jetplasma.com"]
["\n稷以科技软件更新要求\n"]
["设备型号","Triton160"]
["目前版本号","1.40.0.0",null,"提交需求时间","2018-08-30"]
["  更新要求1：                                                                                   "]
["添加射频功率调节系数，使得实际射频功率=设定射频功率*射频功率调节系数，要求如下：\n1.射频功率调节系数只在后台操作，用户UI上无显示；\n2.射频功率调节系数大小范围：0.1-10，默认设定值为1.0；\n3.用户界面多处反映实际射频功率的位置做修改，具体要求见PPT。"]
["  更新要求2：                                                                                 "]
["添加气体流量调节系数，使得实际气体流量=设定气体流量*气体流量调节系数，要求如下：\n1.气体流量调节系数只在后台操作，用户UI上无显示；\n2.气体流量调节系数大小范围：0.1-10，默认设定值为1.0；\n3.用户界面多处反映实际气体流量的位置做修改，具体要求见PPT。"]