{"text_format":"2","workbook":"xlsx","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"charts":0,"images":2,"macros":0,"external_links":0,"defined_names":0,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":12,"n_cols":4,"rows_kept":12,"cut":false,"hidden":false,"merged":[]}
["序号","项目","实现分类","可行性"]
[1,"新产品系统自动绑定Recipe","MES"]
[2,"已有型号固定机台作业，在其它机台上不可作业,报警","MES"]
[3,"机台具备Online功能（必须机台自动带档作业）、Offline功能（可手动作业）","机台"]
[4,"手动/自动识别机台卡塞RF ID或者条形码调档","机台&MES"]
[5,"当站已系统读取，不可重复读取作业（产品异常工程处理后变更系统除外）","机台&MES"]
[6,"定期监控数据上传，若超出监控时间无数据上传机台锁定不允许作业(当前Run作业完)","机台&MES"]
[7,"机台Recipe 程序名可上传MES系统（上传格式）并可查看","机台&MES"]
[8,"机台报警、待料(机台正常，但未作业)、Run时间状况（正常运行时间）可连动稼动率系统（每10分钟统计异常率）","机台&MES"]
[9,"物料使用状况可查看（用量、切换时间点、使用片数）","机台&MES"]
[10,"作业完成时间、绑定明细或制程记录上抛SERVER（提供文件类型、模板）","机台&MES"]
[11,"机台自动带档方式及Check in&Check Out，优先方案二","机台&MES"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}